{"text_format":"5","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"props":{"creator":"Opher Ganel","last_modified_by":"Opher Ganel"},"not_rendered":{"external_links":1},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":190,"n_cols":11,"rows_kept":190,"merged":[[0,5,0,6],[50,5,50,6],[100,5,100,6],[130,0,130,1],[131,1,131,2],[139,0,139,1],[143,2,143,3],[143,4,143,5],[155,0,155,2],[155,4,155,7],[156,0,156,1],[156,4,156,6],[157,0,157,1],[157,4,157,6],[158,0,158,1],[158,4,158,6],[159,0,159,1],[159,4,159,6],[160,0,160,1],[160,4,160,6],[161,0,161,1],[161,4,161,6],[162,0,162,1],[162,4,162,6],[163,0,163,1],[163,4,163,6],[164,0,164,1],[164,4,164,6],[165,0,165,1],[165,4,165,6],[166,0,166,1],[166,4,166,6],[167,0,167,1],[167,4,167,6],[168,0,168,1],[168,4,168,6],[169,0,169,1],[169,4,169,6],[170,0,170,1],[170,4,170,6],[171,0,171,1],[171,4,171,6],[172,0,172,1],[172,4,172,6],[173,0,173,1],[173,4,173,6],[174,0,174,1],[174,4,174,6],[175,0,175,1],[175,4,175,6],[176,0,176,1],[176,4,176,6],[177,0,177,1],[177,4,177,6],[178,0,178,1],[178,4,178,6],[179,0,179,1],[179,4,179,6],[181,0,181,1],[183,0,183,4],[184,0,184,4],[185,0,185,4],[186,0,186,4],[187,0,187,4],[188,0,188,4],[189,0,189,4]],"headers":{"header":["","CREAM Weight Budget (Alternate baseline, strip SCNs, HPDs)"],"footer":["","Page"]},"flags":["formulas_cached_only"]}
["Detector","Material","r","l_int","Shape","Thickness",null,"Top z","Top width","Bot width","Mass"]
[null,null,"g/cm^3","cm",null,"cm","l_int","cm","cm","cm","kg"]
[]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,95.18176000000001,120,120,0.1609344]
["QDET 1X","BC408",1.032,79.457,"Box",0.5,0.0062927117812149975,95.17668,120,120,7.4304000000000014]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,94.67668,120,120,0.1609344]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,94.6716,120,120,0.1609344]
["QDET 1Y","BC408",1.032,79.457,"Box",0.5,0.0062927117812149975,94.66651999999999,120,120,7.4304000000000014]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,94.16651999999999,120,120,0.1609344]
["Clearance",{"$nulls":4},0.3175,null,94.16143999999998,125,125]
["TRD 1","Foam",0.05,1640,"Box",35,0.021341463414634148,93.84393999999999,125,125,37.7]
["Clearance",{"$nulls":4},0.3175,null,58.84393999999999,125,120]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,58.52643999999999,120,120,0.1609344]
["QDET 2X","BC408",1.032,79.457,"Box",0.5,0.0062927117812149975,58.52135999999999,120,120,7.4304000000000014]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,58.02135999999999,120,120,0.1609344]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,58.01627999999999,120,120,0.1609344]
["QDET 2Y","BC408",1.032,79.457,"Box",0.5,0.0062927117812149975,58.01119999999999,120,120,7.4304000000000014]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,57.51119999999999,120,120,0.1609344]
["Clearance",{"$nulls":4},0.3175,null,57.50611999999999,125,125]
["TRD 2","Foam",0.05,1640,"Box",35,0.021341463414634148,57.188619999999986,125,125,37.7]
["Clearance",{"$nulls":4},0.3175,null,22.18861999999999,125,125]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,21.87111999999999,76,76,0.064552576]
["S0 (pixels)","BC408",1.032,79.457,"Box",1,0.012585423562429995,21.86603999999999,76,76,5.960832000000001]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,20.86603999999999,76,76,0.064552576]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,20.86095999999999,74.2,74.2,0.06153103264000002]
["SCN 1X","BC408",1.032,79.457,"Box",0.2,0.002517084712485999,20.855879999999992,74.2,74.2,1.1363640960000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,20.655879999999993,74.2,74.2,0.06153103264000002]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,20.650799999999993,74.2,74.2,0.06153103264000002]
["SCN 1Y","BC408",1.032,79.457,"Box",0.2,0.002517084712485999,20.645719999999994,74.2,74.2,1.1363640960000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,20.445719999999994,74.2,74.2,0.06153103264000002]
["T1","Graphite",2.1,41.09357142857143,"Trpzoid",9.5,0.23117971180754723,20.440639999999995,73.60281801654307,62.800000000000004,92.9900874129115]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,10.940639999999997,62.800000000000004,62.800000000000004,0.044076355840000005]
["SCN 2X","BC408",1.032,79.457,"Box",0.2,0.002517084712485999,10.935559999999997,62.800000000000004,62.800000000000004,0.8140085760000002]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,10.735559999999998,62.800000000000004,62.800000000000004,0.044076355840000005]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,10.730479999999998,62.800000000000004,62.800000000000004,0.044076355840000005]
["SCN 2Y","BC408",1.032,79.457,"Box",0.2,0.002517084712485999,10.725399999999999,62.800000000000004,62.800000000000004,0.8140085760000002]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,10.5254,62.800000000000004,62.800000000000004,0.044076355840000005]
["T2","Graphite",2.1,41.09357142857143,"Trpzoid",9.5,0.23117971180754723,10.52032,62.14781916984001,52,65.15695286225213]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,1.02032,52,52,0.030219904000000002]
["SCN Time X","BC408",1.032,79.457,"Box",0.5,0.0062927117812149975,1.01524,52,52,1.3952640000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,0.5152399999999999,52,52,0.030219904000000002]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,0.51016,52,52,0.030219904000000002]
["SCN Time Y","BC408",1.032,79.457,"Box",0.5,0.0062927117812149975,0.50508,52,52,1.3952640000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,0.00508,52,52,0.030219904000000002]
["Abs 1","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,0,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-0.35,50,50,0.027940000000000003]
["Cal SCN 1","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-0.35507999999999995,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-0.40507999999999994,50,50,0.027940000000000003]
["Abs 2","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-0.4101599999999999,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-0.76016,50,50,0.027940000000000003]
["Detector","Material","r","l_int","Shape","Thickness",null,"Top z","Top width","Bot width","Mass"]
[null,null,"g/cm^3","cm",null,"cm","l_int","cm","cm","cm","kg"]
[]
["Cal SCN 2","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-0.7652399999999999,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-0.81524,50,50,0.027940000000000003]
["Abs 3","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-0.8203199999999999,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-1.1703199999999998,50,50,0.027940000000000003]
["Cal SCN 3","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-1.1753999999999998,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-1.2253999999999998,50,50,0.027940000000000003]
["Abs 4","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-1.2304799999999998,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-1.5804799999999997,50,50,0.027940000000000003]
["Cal SCN 4","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-1.5855599999999996,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-1.6355599999999997,50,50,0.027940000000000003]
["Abs 5","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-1.6406399999999997,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-1.9906399999999995,50,50,0.027940000000000003]
["Cal SCN 5","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-1.9957199999999995,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-2.0457199999999993,50,50,0.027940000000000003]
["Abs 6","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-2.0507999999999993,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-2.4007999999999994,50,50,0.027940000000000003]
["Cal SCN 6","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-2.4058799999999994,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-2.455879999999999,50,50,0.027940000000000003]
["Abs 7","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-2.460959999999999,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-2.8109599999999992,50,50,0.027940000000000003]
["Cal SCN 7","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-2.816039999999999,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-2.866039999999999,50,50,0.027940000000000003]
["Abs 8","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-2.871119999999999,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-3.221119999999999,50,50,0.027940000000000003]
["Cal SCN 8","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-3.226199999999999,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-3.276199999999999,50,50,0.027940000000000003]
["Abs 9","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-3.281279999999999,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-3.631279999999999,50,50,0.027940000000000003]
["Cal SCN 9","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-3.636359999999999,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-3.6863599999999987,50,50,0.027940000000000003]
["Abs 10","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-3.6914399999999987,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-4.041439999999999,50,50,0.027940000000000003]
["Cal SCN 10","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-4.046519999999999,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-4.096519999999999,50,50,0.027940000000000003]
["Abs 11","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-4.1015999999999995,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-4.451599999999999,50,50,0.027940000000000003]
["Cal SCN 11","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-4.4566799999999995,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-4.506679999999999,50,50,0.027940000000000003]
["Abs 12","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-4.51176,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-4.861759999999999,50,50,0.027940000000000003]
["Cal SCN 12","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-4.86684,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-4.91684,50,50,0.027940000000000003]
["Abs 13","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-4.92192,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-5.27192,50,50,0.027940000000000003]
["Cal SCN 13","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-5.277,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-5.327,50,50,0.027940000000000003]
["Abs 14","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-5.33208,50,50,16.887500000000003]
["Detector","Material","r","l_int","Shape","Thickness",null,"Top z","Top width","Bot width","Mass"]
[null,null,"g/cm^3","cm",null,"cm","l_int","cm","cm","cm","kg"]
[]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-5.68208,50,50,0.027940000000000003]
["Cal SCN 14","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-5.68716,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-5.73716,50,50,0.027940000000000003]
["Abs 15","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-5.742240000000001,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-6.09224,50,50,0.027940000000000003]
["Cal SCN 15","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-6.097320000000001,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-6.147320000000001,50,50,0.027940000000000003]
["Abs 16","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-6.152400000000001,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-6.502400000000001,50,50,0.027940000000000003]
["Cal SCN 16","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-6.507480000000001,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-6.557480000000001,50,50,0.027940000000000003]
["Abs 17","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-6.562560000000001,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-6.912560000000001,50,50,0.027940000000000003]
["Cal SCN 17","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-6.917640000000001,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-6.967640000000001,50,50,0.027940000000000003]
["Abs 18","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-6.972720000000002,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-7.322720000000001,50,50,0.027940000000000003]
["Cal SCN 18","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-7.327800000000002,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-7.3778000000000015,50,50,0.027940000000000003]
["Abs 19","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-7.382880000000002,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-7.7328800000000015,50,50,0.027940000000000003]
["Cal SCN 19","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-7.737960000000002,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-7.787960000000002,50,50,0.027940000000000003]
["Abs 20","Tungsten",19.3,9.585,"Box",0.35,0.03651538862806468,-7.793040000000002,50,50,16.887500000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-8.143040000000003,50,50,0.027940000000000003]
["Cal SCN 20","BC408",1.032,79.457,"Box",0.05,0.0006292711781214998,-8.148120000000002,50,50,0.12900000000000003]
["Wrap","Teflon",2.2,49.3,"Sheet",0.00508,0.0001030425963488844,-8.198120000000003,50,50,0.027940000000000003]
["Additional items"]
["Detector","61-pixel HPD/2\" PMT",null,"Plastic","Gas","Elctrncs","Mountng","Total"]
["QDET",40,16,29.82,null,13.635,23.48,82.935]
["TRD",{"$nulls":3},30,15.1,10,55.1]
["S0",24,12,10,null,4.34,null,26.34]
["Target",22,11,6,null,4.34,null,21.34]
["Cal",20,10,6,null,8.68,4.2,28.88]
["Total mass",null,49,51.82,30,46.095000000000006,37.68000000000001,214.595]
[]
["Angle"]
["deg","rad"]
[30,0.5235987756666667]
[]
["Detector","Margin","Thickness",null,"Mass (kg)"]
[null,null,"(cm)","(l_int)","Bare","Total","Margin","Tot+mrg"]
["QDET",null,3.0609599999999997,0.0389927818434766,33.92048281600001,116.855482816,29.213870704,146.06935352]
["TRD",null,71.27000000000001,0.042682926829268296,75.4,130.5,14.500000000000007,145]
["S0 (pixels)",null,1.01016,0.012791508755127764,6.089937152,32.429937152,8.107484288,40.53742144]
["Target SCN",null,1.86096,0.023890273568560605,4.323174897920001,25.66317489792,6.41579372448,32.0789686224]
["Target C",null,19,0.46235942361509447,158.14704027516365,158.14704027516365,1.5974448512642896,159.74448512642795]
["  Target",null,20.86096,0.48624969718365507,162.47021517308366,183.81021517308363,8.013238575744289,191.82345374882792]
["  Cal",null,8.203200000000002,0.7470148999776784,341.4476000000002,370.3276000000002,25.9207157894737,396.2483157894739]
["Cal module",null,30.07432,1.2460561059164612,510.00775232508386,586.5677523250838,42.041438653217995,628.6091909783019]
["CREAM",null,104.40528,1.327731814589206,619.3282351410838,833.9232351410838,85.75530935721801,919.6785444983018]
[]
["McMurdo full-up",{"$nulls":3},"ULDB full-up"]
[{"$nulls":8},"New limits"]
["Gross inflation",null,4310,{"$nulls":5},"(unofficial)"]
["Free lift (12% gross load)",null,461.7857142857143]
["Gross load",null,{"v":3848.214285714286,"d":"3848.2"}]
["Balloon weight",null,1628]
["Zero-Pressure launch limit",null,{"v":2220.214285714286,"d":"2220.2"},null,"Super-Pressure launch limit",null,null,1590.9,2045.4]
["Terminate package",null,127,null,"Flight train",null,null,428.2,428.2]
["Parachute",null,230,null,"Inst.&mission supp. Eq.",null,null,151.4,151.4]
["Pin weight",null,{"v":1863.2142857142858,"d":"1863.2"},null,"Ballast and hopper",null,null,237.7,237.7]
["Inst.&mission supp. Eq.",null,243,null,"Crush pad",null,null,25,25]
["Ballast and hopper",null,237.7]
["Crush pad",null,25]
["Remaining for experiment",null,{"v":1357.5142857142857,"d":"1357.5"},null,"Remaining for experiment",null,null,748.6000000000001,1203.1000000000001]
["Rotator",null,{"v":68.18181818181817,"d":"68.2"},null,"Rotator",null,null,{"v":68.18181818181817,"d":"68.2"},{"v":68.18181818181817,"d":"68.2"}]
["Thermal",null,50,null,"Thermal",null,null,50,50]
["Power system",null,119.7,null,"Power system",null,null,310,310]
["Gondola (support)",null,200,null,"Gondola (support)",null,null,200,200]
["Allowed science wt",null,{"v":919.6324675324676,"d":"919.6"},null,"Allowed science wt",null,null,{"v":120.41818181818189,"d":"120.4"},{"v":574.9181818181819,"d":"574.9"}]
["QDET",null,{"v":146.06935352,"d":"146"},null,"QDET",null,null,146.06935352,{"v":146.06935352,"d":"146"}]
["TRD",null,145,null,"TRD",null,null,145,145]
["CAL",null,{"v":628.6091909783019,"d":"628.6"},null,"CAL",null,null,{"v":628.6091909783019,"d":"628.6"},{"v":628.6091909783019,"d":"628.6"}]
["CREAM sci w/conting",null,{"v":919.6785444983018,"d":"919.7"},null,"CREAM sci w/conting",null,null,{"v":919.6785444983018,"d":"919.7"},{"v":919.6785444983018,"d":"919.7"}]
[]
["Margin",null,{"v":-0.04607696583423149,"d":"-0.0"},null,"Margin",null,null,{"v":-799.2603626801199,"d":"-799.3"},{"v":-344.7603626801199,"d":"-344.8"}]
[]
["Modifications"]
[]
["1. Reduced target thickness to 9.5 cm each"]
["2. Reduced opening angle to 30 degrees"]
["3. Reduced teflon/tedlar to 2 mil thickness"]
["4. Reduced calorimeter to 50 cm x 50 cm"]
["5. Reduced TRD active areas to 120 cm x 120 cm"]
["6. Reduced QDET to 120 cm x 120 cm x 0.5 cm"]
["7. Wrappings of QDET are included in Mounting"]